No. CeNS/2016-17/Admin/WO/92

Date : 10.01.2017

|  |
| --- |
| **REQUEST FOR QUOTATION** |

Dear Sirs,

The Centre invites quotations for Additional pipeline for Bore well in Shivanapura site as detailed in Annexure :

The quotation in the prescribed format may be addressed and sent to the Administrative Officer, Centre for Nano and Soft Matter Sciences, PB No. 1329, Jalahalli, Bangalore – 560 013 so as to reach on or before 17.01.2017.

Terms and Condition :

* The rates quoted shall be exclusive of all taxes which will be paid extra
* Incomplete quotations are liable to be rejected.
* Advance payment will be considered only against progress of work, subject to a maximum of 70% of the total approved cost mentioned in Work Order. Final payment will be based on measurements and payment shall be made by way of NEFT/RTGS after satisfactory work completion.
* The Centre reserves the right to consider the quotations in full or part, without assigning any reasons thereof.
* VAT Service Tax and PAN Registration should be clearly indicated in the Quotation/Invoice.

Sd/-

Administrative Officer

**ANNEXURE**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl No.** | **Description of the Work** | **Approx Quantity** | **Rate**  **(Rs.)** | **Amount**  **(Rs.)** |
| 1. | Earth excavation for foundations of buildings, water supply, sanitary lines and electrical conduits either in pits or in trenches 1.5m and above in width, in hard soil not exceeding 1.5m in depth including dressing the bottom and sides of pits and trenches, stacking the excavated soil clear from edges of excavation with lead up to 50m. after breaking clods complete as per specifications.  BR 15-16/PG-05/1-2.4  1000m x 0.30x0.60 = 180.0cum | 180 Cum |  |  |
| 2. | Providing and fixing Chlorinated Poly Venyl Chloride (CPVC) Pipes conforming to IS 15778, having thermal stability for hot and cold water supply including all cpvc fittings this includes jointing of pipes and fittings with one step solvent cement and testing of joints complete  BR 15-16/PG-97/13.87.6  All round campus from existing line = 990rmtr | 990Rmtr |  |  |
| 3. | Providing and fixing Chlorinated Venyl Chloride (CPVC) Pipes conforming to IS 15778, having thermal stability for hot and cold water supply including all cpvc fittings this includes jointing of pipes and fittings with one step solvent cement & testing of joints complete  BR 15-16/PG-97/13.87.3 for stand pipes raising = 30rmts | 30 Rmtr |  |  |
| 4. | Providing and fixing cpvc gate valves for ring main pipe line at necessary place at operating levels including cost of materials and labour. market rate | 7 Nos. |  |  |
| 5. | Providing and fixing HDPE Claw Foot Valves for gardening and sprinklers including cost of materials and labour market rate. | 30 Nos. |  |  |
| 6. | Providing and fixing to wall, floor, and ceiling medium density polyethylene pipes 6.00 kgs/Sq.cm working pressure 160mm outside diameter with cost of materials and labour.  BR 15-16/PG-93/I-13.70.7 for puddle sleeves operating gatevalves | 4 Rmtr |  |  |

Seal and Signature of the Firm

Date :