No. CeNS/2017-18/Admin/WO/ Date : 16.05.2017

|  |
| --- |
| **REQUEST FOR QUOTATION** |

To,

M/s.

Dear Sirs,

The Centre invites quotations for the below mentioned work. Details are as under :-

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl. No** | **Description** | **Area****(sq-ft)** | **RATE** | **Total Amount****(Rs.)** |
| 1. | **CHEMICAL STORE – 1 No.** | 20’(L) x 20’ (W) x 10’ (H)400 Sq ft. |  |  |
| 1a. | Fabrication of MS-Structure for use as Chemical Store measuring 20’ (Length) x 20’ (Width) x 10’ (Height) using high strength sheets along with insulation designed to absorb heat and noise.  |
| 1b. | Double door – 3’ x 7’ each with insulation and canopy with fixed glass of 18” (Width) x 24” (Length) for clear vision. | 3’ x 7’18” (W) x 24” (L) glass |  |  |
| 1c. | Flooring – Cement concrete with finish or optionally, fabricated with MS-Steel and chequered plates to withstand heavy storage items without any damage. |  |  |  |
| 1d. | Provision of 4 windows 4’ (L) x 5’ (W) and ventilators to be made (Powder coated 2 track aluminium windows with safety grills and canopy) |  |  |  |
| 4. | All electrical wiring to be done with safety standards concealed within PVC casing with 2.5 sq mm wiring for inclusion of sufficient number of lights, exhaust fans and external lighting |  |  |  |
| 2 | **OFFICE SPACES – 2 Nos.** | 12”(L) x 10’(W) x 10’(H) |  |  |
| 2a. | Same specification as above, inclusive of pre - laminated MDF board for walls and insulation for absorption of heat and noise.  | 120 Sq ft. x 2 units |  |  |
| 2b. | Doors – 4’ x 7’ with insulation | 4’ x 7’ |  |  |
| 2c. | Windows – 3’ x 4’ – 2 Nos.(Two track aluminium windows with safety grills and canopy ( 2 Nos. each) | 3’ x 4’ – 2 Nos. each |  |  |
| 3. | Electrical - All electrical wiring to be done with 3 wire (phase, neutral & earth) with 2.5 sq mm wire fittings for sufficient number of switches, lights, exhaust fans, and external lighting 15 amp socket, MCB in all structures.  |  |  |  |
| 4. | Painting – Metal priming to withstand rust + Enamel painting exterior – 2 coats. wherever necessary |  |  |  |
| 5. | Civil work of demolition of existing concrete structure on site and clearing of debris | 300 Sq ft approx. |  |  |

Terms & conditions:

* The quotations should be accompanied with a drawing (floor plan) indicating elevation and measurements.
* Incomplete quotations are liable to be rejected.
* Payment shall be made by way of NEFT/RTGS after satisfactory work completion.
* The Centre reserves the right to consider the quotations in full or in part, without assigning any reasons thereof.
* VAT Service Tax and PAN Registration should be clearly indicated in the Quotation/Invoice.

The sealed quotation may be addressed and sent to the Administrative Officer, Centre for Nano and Soft Matter Sciences, PB No. 1329, Jalahalli, Bangalore – 560 013 so as to reach on or before 15.06.2017

 Yours sincerely,

 Administrative Officer