|  |
| --- |
| Specification Spot extractor: |

**Alsident Spot Extractor**

1. Alsident System 75 Exhaust Arm (75-6555-3-5) Ceiling Mounted 3 White joints, Reach: 1230 mm= 2 nos are required
2. Transparent Hood 1-7535-5 - dia 385 mm- 2 nos are required
3. Ceiling column : total 3000mm. (Side Connection)

**Blower & Ducting**

1. Centrifugal Blower (0.5 HP) with DOL Starter in cluster of 2 nos. of spot extractor
2. PP + FRP Ducting = total 200 square feet is required

