**SPECIFICATION S FOR THE DUAL FREQUENCY ULTRASONIC BATH**

Max. working volume : Around 20 liters

Internal dimensions WxDxH : 300/300/300 mm

External dimensions WxDxH : 500/550/936

frequency dual : 25/45 kHz

Mains voltage VAC : 230V 50Hz

Total power consumption : 2000W

Effective ultrasound output : 480 (25/45kHz]

Ultrasound pulse mode W : 480 (25/45kHz]

Max. peak ultrasound output : 1920 (25/45kHz)

Ultrasound pulse mode W : 920 (25/45kHz)

Effective ultrasound output : 600W

Max. peak ultrasound output : 2400W

Heating Power : 1400W

**Accessories :**

Sound Protection Lid

Stainless Steel Basket

Basket insert Stainles steel

Features:

1. Sweep-function for optimum sound field distribution
2. Switchable Pulse-function for increasing the peak ultrasonic performance
3. Dynamic-function: The Sweep- and Pulse-functions run alternately on an automatic basis.
4. Individual time and temperature regulation
5. High user safety with automatic safety shutdown
6. Caster wheels for easy movement of the bath
7. Warranty should be 12 months from the date of installation and 24 months free of cost service support to be provided