**Technical Specifications for Electric vertical roll press machine**

* Roller diameter : 96mm
* Ra : >0.8um
* Press gap: 0-2mm adjustable or better.
* Rolling width :150 mm
* Rolling speed: 0～40mm/s adjustable or better.
* Temperature up to 1200C or better.
* Temperature accuracy ***±***10
* Roller material: Hardness should be on par with HRC62.
* Size: L385mm\*W245mm\*H355mm or smaller.
* Heat, rollingtemperature could be regulated and should be digitally displayed.
* Weight : below 65 kg
* Power and voltage: Watt :100W, Voltage : 220V
* Warranty- 1 Year with life time support.
* CE and ISO certification
* At least should have 5 installations in India.